1. Visit the official website and click on "Download" > "Firmware Upgrade" to access the download page.

图形用户界面, 应用程序

描述已自动生成

2. Download the corresponding firmware based on your product model.

图形用户界面, 应用程序, Teams

描述已自动生成

3. Extract the appropriate firmware and launch the BootLoader upgrade tool.

图形用户界面, 应用程序

描述已自动生成

4. Connect your device to the computer, ensuring that the device can control the cursor.

5. Click "OneKeyUpdate."

图形用户界面, 应用程序, 电子邮件

描述已自动生成

6. Wait for the installation to complete. After receiving the "Burn Success" prompt, you can close the window and exit.

图片包含 文本

描述已自动生成

7. You can test the pressure sensitivity in driver versions 4.2.3 and above.

图形用户界面

描述已自动生成

If you need any further assistance, please dont hesitate to contact us:

Website: www.ugee.com

Email: service@ugee.com